>> MIB - Management Information Base
>> Table: igmpDstListTable - (.1.3.6.1.4.1.272.4.5.51.9.1)
Description: An entry (conceptual row) in the igmpDstListTable.
igmpDstListTable
OID | Name | Type | Access
.1 | GroupAddress | IpAddress | R
.2 | Address | IpAddress | R
.3 | IfIndex | InterfaceIndex | R
.4 | Hwaddr | PhysAddress | R
.5 | SourceAddress | IpAddress | R
.6 | Timer | TimeTicks | R
GroupAddress
The igmpCacheAddress/igmpSrcListAddress value (multicast-group-address) of the related igmpCacheTable/igmpSrcListTable entry.
Address
The IP-address of the host/listener specified by this entry.
IfIndex
The igmpCacheIfIndex/igmpSrcListIfIndex value (interface-index) of the related igmpCacheTable/igmpSrcListTable entry. Range: 1 to 2147483647
Hwaddr
The media-dependent physical address of the host/listener specified by this entry. Length: 0 to 65535
SourceAddress
Either 0 (ASM-case, referring to igmpCacheTable entry) or igmpSrcListHostAddress (multicast-sender) of related igmpSrcListTable entry (SSM-case).
Timer
The time when this entry will be aged out.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH