>> MIB - Management Information Base
>> Table: ipDynDnsProviderTable - (.1.3.6.1.4.1.272.4.5.26.1)
Description:
ipDynDnsProviderTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Name | DisplayString | RW
.3 | Server | DisplayString | RW
.4 | Path | DisplayString | RW
.5 | Port | INTEGER | RW
.6 | Protocol | ENUM | D
.7 | MinWait | INTEGER | RW
.8 | Verification | ENUM | RW
.9 | UpdateInterval | INTEGER | RW
.10 | Server6 | DisplayString | RW
.11 | SupportsSSL | ENUM | RW
.12 | MoreInfo | DisplayString | RW
Index
Index of provider entry
Name
Name of dyn-dns provider Length: 0 to 255
Server
Server for publishing IPv4 addresses Length: 0 to 255
Path
Path for publishing (shared for IPv4/IPv6-address-case) Length: 0 to 255
Port
Port used for publishing. Ignored if URL is explicitly adjusted for HTTP/HTTPS.
Protocol
Publishing protocol used by provider Enumerations: dyndns (1) stat-dyndns (2) ods (3) hn (4) dyns (5) gnudip-html (6) gnudip-tcp (7) cust-dyndns (8) dnsexit (9) dyndnss (10) dyndns2 (11) delete (100)
MinWait
Minimal time to wait between ip updates
Verification
Disables the up-to-date check (IP address versus FQDN verification) if needed for specific services. Enumerations: enabled (1) disabled (2)
UpdateInterval
Optional update interval in case of static IP address.
Server6
Server for publishing IPv6 addresses Length: 0 to 255
SupportsSSL
Indicates that HTTPS(SSL) is supported and can be selected via 'ipPublishUseSSL' setting. Enumerations: yes (1) no (2)
MoreInfo
Contains for example the link to the providers homepage. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH