>> MIB - Management Information Base
>> Table: atmQosVccTable - (.1.3.6.1.4.1.272.4.16.19.1)
Description: An entry in the table, containing ATM QoS parameters about a particular virtual connection.
atmQosVccTable
OID | Name | Type | Access
.1 | AtmIfIndex | Integer32 | RW
.2 | Vpi | INTEGER | RW
.3 | Vci | INTEGER | RW
.4 | Service | ENUM | D
.5 | OutPcr | Integer32 | RW
.6 | OutScr | Integer32 | RW
.7 | OutMbs | Integer32 | RW
.8 | OutMcr | Integer32 | RW
AtmIfIndex
The interface index of the associated ATM hardware.
Vpi
The VPI value of this Virtual Channel Connection. Range: 0 to 255
Vci
The VCI value of this Virtual Channel Connection. Range: 0 to 65535
Service
The ATM service category of this virtual circuit connection: cbr vbr vbr2 vbr3 VBR1 + Best Effort vbr-rt real-time vbr2-rt real-time vbr3-rt real-time ubr Best Effort ubr2 Best Effort abr delete Enumerations: cbr (1) vbr (2) vbr3 (4) ubr (8) delete (20)
OutPcr
Output Peak Cell Rate (PCR) in bps.
OutScr
Output Sustained Cell Rate (SCR) in bps.
OutMbs
Output Maximum Burst Size (MBS) in Bytes, only for atmQosVccService vbr-rt(2) and vbr-nrt(3) (ATM service service category VBR).
OutMcr
Output Minimum Cell Rate (MCR) in bps for connection with vbr-nrt(3).

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH