>> MIB - Management Information Base
>> Table: biboBrrpRouterStatsTable - (.1.3.6.1.4.1.272.4.40.2.1)
Description: An entry in the table, containing statistics information about a given virtual router.
biboBrrpRouterStatsTable
OID | Name | Type | Access
.1 | VrId | INTEGER | R
.2 | IfIndex | INTEGER | R
.3 | BecomeMaster | Counter | R
.4 | AdvertiseRcvd | Counter | R
.5 | AdvertiseIntervalErrors | Counter | R
.6 | AuthFailures | Counter | R
.7 | IpTtlErrors | Counter | R
.8 | InvalidTypePktsRcvd | Counter | R
.9 | InvalidAuthType | Counter | R
.10 | AuthTypeMismatch | Counter | R
.11 | PacketLengthErrors | Counter | R
.12 | ChecksumErrors | Counter | R
.13 | VersionErrors | Counter | R
VrId
This object contains the Virtual Router Identifier (VRID). Range: 1 to 255
IfIndex
The index of the virtual interface used by the virtual router.
BecomeMaster
The total number of times that this virtual router's state has transitioned to MASTER.
AdvertiseRcvd
The total number of BRRP advertisements received by this virtual router.
AdvertiseIntervalErrors
The total number of BRRP advertisement packets received for which the advertisement interval is different than the one configured for the local virtual router.
AuthFailures
The total number of BRRP packets received that do not pass the authentication check.
IpTtlErrors
The total number of BRRP packets received by the virtual router with IP TTL (Time-To-Live) not equal to 255.
InvalidTypePktsRcvd
The number of BRRP packets received by the virtual router with an invalid value in the 'type' field.
InvalidAuthType
The total number of packets received with an unknown authentication type.
AuthTypeMismatch
The total number of packets received with 'Auth Type' not equal to the locally configured authentication method (`brrpOperAuthType').
PacketLengthErrors
The total number of packets received with a packet length less than the length of the BRRP header.
ChecksumErrors
The total number of BRRP packets received with an invalid BRRP checksum value.
VersionErrors
The total number of BRRP packets received with an unknown or unsupported version number.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH