>> MIB - Management Information Base
>> Table: mpsParallelRingingTable - (.1.3.6.1.4.1.272.4.53.6.16.1)
Description: This table contains information about parallel ringing feature. If the extension is called an additional parallel call we be initiated.
mpsParallelRingingTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Extension | ExtensionIndexOrZero | RW
.3 | Facilities | ENUM | RW
.4 | Number | DisplayString | RW
.5 | AdminStatus | ENUM | D
Index
A unique value for each parallel ringing entry.
Extension
This variable contains the extension for this parallel ringing entry. Reference to mpsExtensionIndex in mpsExtensionTable. Range: 0 to 65535
Facilities
mpsPRFacilities: This value decides which number will be used for the parallel call: pr-number: the configured number (mpsPRNumber) mobile-number: the mobile number (mpsUserMobileNumber in mpsUserTable) home-number: the home number (mpsUserHomeNumber in mpsUserTable) Enumerations: pr-number (1) mobile-number (2) home-number (3)
Number
This variable contains the digits of the parallel ringing number. Length: 0 to 24
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH