>> MIB - Management Information Base
>> Table: phoneIfRingTable - (.1.3.6.1.4.1.272.4.15.1.3.1)
Description: The phoneIfRingTable the contains configuration information for ringing signals.
phoneIfRingTable
OID | Name | Type | Access
.1 | Index | RingTabIndex | RW
.2 | InternCadence | CadenceString | RW
.3 | ExternCadence | CadenceString | RW
.4 | InquiryCadence | CadenceString | RW
.5 | InternRecallCadence | CadenceString | RW
.6 | ExternRecallCadence | CadenceString | RW
.7 | InternCallBackCadence | CadenceString | RW
.8 | ExternCallBackCadence | CadenceString | RW
.9 | InternDoorCadence | CadenceString | RW
.10 | AlarmCadence | CadenceString | RW
.11 | AnnouncementCadence | CadenceString | RW
.12 | IntercomCadence | CadenceString | RW
.13 | ChiefCadence | CadenceString | RW
.14 | SecretaryCadence | CadenceString | RW
.15 | MwiCadence | CadenceString | RW
.16 | WebServiceCadence | CadenceString | RW
Index
Index of the set of ring cadences.
InternCadence
Ring cadence definition string for an internal call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
ExternCadence
Ring cadence definition string for an external call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
InquiryCadence
Ring cadence definition string for an inquiry call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
InternRecallCadence
Ring cadence definition string for internal recall. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
ExternRecallCadence
Ring cadence definition string for external recall. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
InternCallBackCadence
Ring cadence definition string for internal call back. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
ExternCallBackCadence
Ring cadence definition string for external call back. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
InternDoorCadence
Ring cadence definition string for an internal door call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
AlarmCadence
Ring cadence definition string for an alarm call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
AnnouncementCadence
Ring cadence definition string for an announcement call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
IntercomCadence
Ring cadence definition string for an intercom call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
ChiefCadence
Ring cadence definition string for an chief call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
SecretaryCadence
Ring cadence definition string for an secretary call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
MwiCadence
Ring cadence definition string for a message waiting call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127
WebServiceCadence
Ring cadence definition string for a web service call. For a description of allowed format refer to phoneIfToneDefinitionCadence. Length: 0 to 127

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH