>> MIB - Management Information Base
>> Table: wlanVSSStatsTable - (.1.3.6.1.4.1.272.4.46.31.1)
Description: Shows WLAN VSS statistics
wlanVSSStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | ClearCounter | ENUM | RW
.3 | Current | INTEGER | R
.4 | SoftTotalDenied | INTEGER | R
.5 | BSMovements | INTEGER | R
.6 | TotalDenied | INTEGER | R
IfIndex
Unique VSS index of a Broadcast VSS.
ClearCounter
The administrative status of the wlanVSSStats entry.
Current
Number of currently associated stations.
SoftTotalDenied
Number of rejected clients due to wlanVSSSoftTotal limit.
BSMovements
Number of clients moved to other band by band steering mechanism.
TotalDenied
Number of rejected clients due to wlanVSSTotal limit.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH