>> MIB - Management Information Base
>> Table: dot11ResourceInfoTable - (.1.2.840.10036.3.1.2.1)
Description: An entry in the dot11ResourceInfo Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11ResourceInfoTable
OID | Name | Type | Access
.1 | OUI | OCTET STRING | R
.2 | Name | DisplayString | R
.3 | ProductName | DisplayString | R
.4 | ProductVersion | DisplayString | R
OUI
Takes the value of an organizationally unique identifier. Length: 3 to 3
Name
A printable string used to identify the manufacturer of the resource. Maximum string length is 128 octets. Length: 0 to 128
ProductName
A printable string used to identify the manufacturer's product name of the resource. Maximum string length is 128 octets. Length: 0 to 128
ProductVersion
Printable string used to identify the manufacturer's product version of the resource. Maximum string length is 128 octets. Length: 0 to 128

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH