>> MIB - Management Information Base
>> Table: ipSifRejectTable - (.1.3.6.1.4.1.272.4.5.31.1)
Description: Contains actually rejected Frames with Source Destination
ipSifRejectTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Source | IpAddress | R
.3 | Destination | IpAddress | R
.4 | Rejects | INTEGER | R
.5 | Silence | INTEGER | R
.6 | Protocol | INTEGER | R
.7 | PortLo | INTEGER | R
.8 | PortHigh | INTEGER | R
Index
The Index for the Reject Entry
Source
The Reject Source for the Entry
Destination
The Reject Destination Index for the Entry
Rejects
Count of rejected frames
Silence
Last reject in seconds
Protocol
The protocol of the rejected Packet
PortLo
The lowest Port rejected
PortHigh
The highest port rejected

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH