>> MIB - Management Information Base
>> Table: wlanDynamicBlacklistTable - (.1.3.6.1.4.1.272.4.46.30.1)
Description: The wlanDynamicBlacklist contains information about stations that are blacklisted as a countermeasure to inappropriate behaviour.
wlanDynamicBlacklistTable
OID | Name | Type | Access
.1 | STAMac | MacAddress | R
.2 | VSSIndex | INTEGER | R
.3 | FirstSeen | Date | R
.4 | LastSeen | Date | R
.5 | Reason | ENUM | RC
.6 | LastRSSI | INTEGER | R
.7 | RowStatus | ENUM | D
STAMac
The MAC address of the station that is blacklisted.
VSSIndex
The SSID the blacklist entry belongs to.
FirstSeen
The 1st time a blacklisted station drew attention.
LastSeen
The last time a blacklisted station drew attention.
Reason
The reason why a station is blacklisted.
LastRSSI
RSSI of station it annoyed last time.
RowStatus
The row status of the blacklist entry. Although the conceptual row is not creatable by the user, one is able to set the row to notInService.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH