>> MIB - Management Information Base
>> Table: mpsSubscriberNumberTable - (.1.3.6.1.4.1.272.4.53.4.1.1)
Description: This table contains information about the call distribution for incoming external calls.
mpsSubscriberNumberTable
OID | Name | Type | Access
.1 | TrunkGroup | TrunkGroupIndex | RW
.2 | Index | SubscriberNumberIndex | RW
.3 | Type | ENUM | RW
.4 | Target | ENUM | RW
.5 | GroupIndex | GroupIndexOrZero | RW
.6 | ExtensionIndex | ExtensionIndexOrZero | RW
.7 | AdminStatus | ENUM | D
TrunkGroup
A unique value for each trunk group index. Range: 1 to 65535
Index
A unique value for each call distribution.
Type
This variable contains the information of the type of number. Enumerations: simple (1) composite (2)
Target
The external number can be assigned to internal teams or subscribers. Enumerations: group (1) extension (2) call-through (3)
GroupIndex
This variable contains the group index, if mpsCallDistributionTargetType=team. Range: 0 to 99
ExtensionIndex
This variable contains the extension index, if mpsCallDistributionTargetType=extension. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH