>> MIB - Management Information Base
>> Table: mpsDoorIntercomTable - (.1.3.6.1.4.1.272.4.53.7.1.1)
Description: This table contains the global information about door intercoms.
mpsDoorIntercomTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | ConnectDTMF | DisplayString | RW
.3 | AdminStatus | ENUM | D
Index
A unique value for each door intercom. Range: 1 to 10
ConnectDTMF
Doorline adapter keycode for call acception. Length: 0 to 24
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH