>> MIB - Management Information Base
>> Table: certStats - (.1.3.6.1.4.1.272.4.26.33.8)
certStats
OID | Name | Type | Access
.1 | certStatCertsConfigured | INTEGER | R
.64 | certCacheStats | ipsec | N
.1 | MemoryUsage | INTEGER | R
.2 | NumEntries | INTEGER | R
.3 | NumCertCacheHit | INTEGER | R
.4 | NumCertCacheMiss | INTEGER | R
.5 | NumCrlCacheHit | INTEGER | R
.6 | NumCrlCacheMiss | INTEGER | R
certStatCertsConfigured
Number of configured certificate entries (opposed to those dynamically learnt by any means during system run).
certCacheStats
description not available
MemoryUsage
Allocated memory by the certificate cache.
NumEntries
Number of entries used in the certificate cache. Range: 0 to 65535
NumCertCacheHit
Number of successful certificate requests from cache. Range: 0 to 65535
NumCertCacheMiss
Number of failed certificate requests from cache. Range: 0 to 65535
NumCrlCacheHit
Number of successful crl requests from cache. Range: 0 to 65535
NumCrlCacheMiss
Number of failed crl requests from cache. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH