>> MIB - Management Information Base
>> Table: httpSessionStatTable - (.1.3.6.1.4.1.272.4.22.3.2.1.1)
Description: This table contains all registered sessions clients.
httpSessionStatTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | R
.2 | State | ENUM | D
.3 | Start | Date | R
.4 | Expiry | Date | R
.5 | Rights | BITS | R
.6 | User | DisplayString | R
.7 | Host | DisplayString | R
.8 | RemoteAddr | IpAddress | R
.9 | AccessClass | ENUM | R
Index
A unique value for each registerd sessions.
State
Status of HTTP session. As long as a session exists in this table its state is active. Setting the session state to delete will cause this entry to be deleted as well as the related session. Enumerations: delete (1) active (2)
Start
Timestamp when the session was started Range: 0 to -1
Expiry
Timestamp when session will expire. This entry is updated every http request received for this session with current time plus httpAdminSessionTimeout. Range: 0 to -1
Rights
The mask contains session rights of authorized user copied over from respective biboAdmLoginHTTPAccessRights table entry. Enumerations: admin (0) fci (1) maint (2) easp (3)
User
Contains the name of the authorized user copied over from the respective biboAdmLogin table entry. Length: 0 to 255
Host
Contains host field from HTTP request header. Length: 0 to 255
RemoteAddr
IP address of client at time of HTTP session initiation. Actually this wouldn't normally change during a session's lifetime but also wouldn't get updated if so.
AccessClass
Contains HTTP access class of authorized user, copied over from biboAdmLoginHTTPAccessClass of respective biboAdmLogin table entry during session initiaition. Enumerations: user (1) admin (2) service (4)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH