>> MIB - Management Information Base
>> Table: wlcAutoWlanIfTable - (.1.3.6.1.4.1.272.4.61.1.38.1)
Description: The wlcAutoWlanIfTable contains all auto configured WLAN interfaces of each WTP with their configured profiles.
wlcAutoWlanIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | WTPIndex | INTEGER | RW
.3 | RadioNo | INTEGER | RW
.4 | ProfIndex | INTEGER | RW
.5 | ClientIndex | INTEGER | RW
Index
Unique index.
WTPIndex
Configured WTP index. See wlcAutoWTPIndex.
RadioNo
Radio number to match.
ProfIndex
Configured WLAN interface profile index. See wlcWlanIfProfileIndex.
ClientIndex
Index pointer to the wlcClientProfileTable.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH