>> MIB - Management Information Base
>> Table: wlcVSSBadAuthAcctTable - (.1.3.6.1.4.1.272.4.61.1.34.1)
Description: The wlcAuthAcct contains some authentication accounting parameters for a wlcVSS.
wlcVSSBadAuthAcctTable
OID | Name | Type | Access
.1 | WlcVSSProfIndex | INTEGER | R
.2 | STAMac | MacAddress | R
.3 | Time1stFail | Date | R
.4 | TimeLastFail | Date | R
.5 | NumFailAttempts | INTEGER | R
.6 | LastRSSI | INTEGER | R
.7 | WTPIndex | INTEGER | R
WlcVSSProfIndex
Reference to wlcVSS entry this authentication accounting information corresponds to.
STAMac
The MAC address of the station the failed authentication attempts are originating from. Length: 6 to 6
Time1stFail
Timestamp of the first failed authentication attempt. This entry is deleted after 1 hour of inactivity. Range: 0 to -1
TimeLastFail
Timestamp of the last failed authentication attempt. Range: 0 to -1
NumFailAttempts
The number of failed authentication attempts from a given station on a given wlcVSS since the first failed authentication attempt within an hour.
LastRSSI
The last RSSI of the station with failing authentication.
WTPIndex
The last WTP a station with failing to authenticate was seen.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH