>> MIB - Management Information Base
>> Table: mpsExtensionCAPITable - (.1.3.6.1.4.1.272.4.53.6.10.1)
Description: This table contains the additional information of the CAPI extension.
mpsExtensionCAPITable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | WakeOnLan | ENUM | D
.3 | MacAddress | MacAddress | RW
Index
A unique value for additional CAPI extension settings. Range: 1 to 65535
WakeOnLan
This value determine if Wake On LAN is off or on. Set to delete, to discard the whole entry. Enumerations: off (1) magic-packet (2) delete (3)
MacAddress
This variable contains the MAC address of the capi extension. Length: 6 to 6

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH