>> MIB - Management Information Base
>> Table: bintecsec - (.1.3.6.1.4.1.272.254)
bintecsec
OID | Name | Type | Access
.1 | AdminCommunity | DisplayString | RW
.2 | ReadCommunity | DisplayString | RW
.3 | WriteCommunity | DisplayString | RW
.5 | RadiusSecret | DisplayString | RW
.6 | HttpPassword | DisplayString | RW
.10 | PublicKey | OCTET STRING | R
.11 | PrivateKey | OCTET STRING | N
.12 | ActMonPassword | DisplayString | RW
AdminCommunity
The Community name used for admin access Length: 0 to 255
ReadCommunity
The Community name used for read-only access. Length: 0 to 255
WriteCommunity
The Community name used for read-write access. Length: 0 to 255
RadiusSecret
The shared secret for RADIUS access. Length: 0 to 255
HttpPassword
The password for HTTP access. Length: 0 to 255
PublicKey
Generated public key for TAF client access
PrivateKey
description not available
ActMonPassword
The password for Activity Monitor access. Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH