>> MIB - Management Information Base
>> Table: ipWalledGardenAddressTable - (.1.3.6.1.4.1.272.4.5.62.6.1)
Description: An entry representing an IP address for which host access authentication is enabled.
ipWalledGardenAddressTable
OID | Name | Type | Access
.1 | DomainOperIndex | INTEGER | R
.2 | Network | IpAddress | R
DomainOperIndex
The parent index in ipWalledGardenDomainOperTable with same value for ipWalledGardenDomainOperIndex.
Network
This object specifies together with ipWalledGardenAddressNetmask the network where hosts can communicate without authorization.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH