>> MIB - Management Information Base
>> Table: biboAdmUsrTrapTable - (.1.3.6.1.4.1.272.4.1.18.1)
Description: The biboAdmUsrTrapTable lists user-defined objects that are used to create traps. These traps are sent locally, but can also be sent to remote hosts using the biboAdmTrapHostTable. Creating entries: Entries are created by assigning the biboATrpObj object a valid object identifier. Deleting entries: Entries are removed by setting the entry's biboATrpStatus object to 'delete'.
biboAdmUsrTrapTable
OID | Name | Type | Access
.1 | Obj | OBJECT IDENTIFIER | RW
.2 | Status | ENUM | D
Obj
The object identifier of an object to use. Each time this object's value changes, a trap is created and sent. Either a single leaf (single variable) or a table (of objects) can be specified.
Status
The status of this entry. Upon creation of a new entry, this object's value is set to 'valid'. Enumerations: valid (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH