>> MIB - Management Information Base
>> Table: ipSifAliasAddressGroupTable - (.1.3.6.1.4.1.272.4.5.47.1)
Description: Defines IP address or interface group alias
ipSifAliasAddressGroupTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | Alias | DisplayString | RW
.3 | Index | INTEGER | R
.4 | Mode | ENUM | D
Id
The unique address group entry ID
Alias
Alias name for the address group entry Length: 0 to 255
Index
The index for the address group entry to be referred by an ipSifAlias entry
Mode
Specifies wether this entry defines an interface or address group Enumerations: interface (1) address (2) delete (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH