>> MIB - Management Information Base
>> Table: mpsExtensionStatusTable - (.1.3.6.1.4.1.272.4.53.6.17.1)
Description: This table contains status information about each extension logged-in in a call-center group (mpsGroupTable).
mpsExtensionStatusTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | R
.2 | EndOfWrapUpTime | Date | R
.3 | ConnectionStatus | ENUM | R
.4 | SumConnectedCalls | Counter32 | R
.5 | ConnectedCalls | Counter32 | R
.6 | SumConnectionTime | INTEGER | R
.7 | ConnectionTime | INTEGER | R
Index
A unique value for each extension. Range: 1 to 65535
EndOfWrapUpTime
This variable contains the end or wrap-up time for this extension, after termination of an incoming call for mpsGroupModeOperation_call_center. Range: 0 to -1
ConnectionStatus
This variable contains the connection status. Enumerations: idle (1) connected (2) ringing (3)
SumConnectedCalls
This variable contains the summary of connected calls since system start.
ConnectedCalls
This value is a copy from mpsExtensionStatusSumConnectedCalls at 0:00h. To get the summary of the connected calls from a day, subtract the mpsExtensionStatusConnectedCalls from mpsExtensionStatusSumConnectedCalls.
SumConnectionTime
This variable contains the summary of time of the connected calls.
ConnectionTime
This value is a copy from mpsExtensionStatusSumConnnectionTime at 0:00h. To get the summary of time of the connected calls from a day, subtract the mpsExtensionStatusConnectionTime from mpsExtensionStatusSumConnectionTime.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH