>> MIB - Management Information Base
>> Table: vmsGlobalStatus - (.1.3.6.1.4.1.272.4.34.1.2)
vmsGlobalStatus
OID | Name | Type | Access
.1 | AccountDir | DisplayString | R
.2 | WaveDir | DisplayString | R
.3 | FileUploadResult | ENUM | RW
AccountDir
This value contains the directory of the account data, This value will be changed by the system. Length: 0 to 255
WaveDir
This value contains the directory of the wave files, This value will be changed by the system. Length: 0 to 255
FileUploadResult
file upload result (error) code: success(1) : the file upload was successful, no-mem-card(2) : no memory card plugged, no-mem-space(3) : no more space available on the memory card, incomp-format(4) : the file format doesn't match the requirements, transfer-error(5) : any transfer error occured during upload, write-protection(6): active write protection on storage device, internal-error(7) : unexpected internal error occured. Enumerations: success (1) no-mem-card (2) no-mem-space (3) incomp-format (4) transfer-error (5) write-protection (6) internal-error (7)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH