>> MIB - Management Information Base
>> Table: systemPhoneOemUserTable - (.1.3.6.1.4.1.272.4.64.6.2.1)
Description: This table contains personal information about OEM system phones. (It must be autosaved because the parameter can be changed by a user).
systemPhoneOemUserTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | Language | ENUM | RW
.3 | AdminStatus | ENUM | D
Index
Reference to the mpsTerminalTable, a unique value for each OEM system phone. Range: 1 to 65535
Language
The current display language of the phone device. Enumerations: german (1) dutch (2) english (3) italian (5) danish (6) spanish (7) swedish (8) french (10) portuguese (11) czech (14) norwegian (16) greek (17) icelandic (20) polish (21) hungarian (22) russian (23) romanian (24) slovak (25)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH