>> MIB - Management Information Base
>> Table: bacEntityRelationTable - (.1.3.6.1.4.1.272.4.60.1.3.1)
Description: One entry in bacEntityRelationTable.
bacEntityRelationTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | PropertyIndex | INTEGER | RW
.3 | EntityType | ENUM | RW
.4 | EntityIndex | INTEGER | RW
.5 | AdminStatus | ENUM | D
Index
The index in this entity relation table. Range: 1 to 65535
PropertyIndex
Index of entry in bacPropertyTable to be referenced. Range: 1 to 65535
EntityType
The type of entity. provider(1) The entity is a provider extension(2) The entity is an extension Enumerations: provider (1) extension (2)
EntityIndex
The index in corresponding entity table. Depending on the used product different entities are addressed: bacEntityRelationEntityType provider: voipProviderTable or mpsTrunkGroupTable bacEntityRelationEntityType extension: voipExtensionTable or mpsTerminalTable Range: 1 to 65535
AdminStatus
If the AdminStatus is set to enabled(1) this entry will be used, if set to disabled(2) it won't be used. You may also delete this entry by changing it to delete(3). Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH