>> MIB - Management Information Base
>> Table: bacAddressTable - (.1.3.6.1.4.1.272.4.60.1.5.1)
Description: One entry in bacAddressTable.
bacAddressTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | PropertyIndex | INTEGER | RW
.3 | IpAddress | IpAddress | RW
.4 | IpNetmask | IpAddress | RW
.5 | Domain | DisplayString | RW
.6 | AdminStatus | ENUM | D
Index
The index in this IP address table. Range: 1 to 65535
PropertyIndex
Index of entry in bacPropertyTable to be referenced. Range: 1 to 65535
IpAddress
The address defining the IP address range.
IpNetmask
The netmask defining the IP address range.
Domain
The domain name defining the address. If empty bacAddressIpAddress and bacAddressIpNetmask is used. Length: 0 to 255
AdminStatus
If the AdminStatus is set to enabled(1) this entry will be used, if set to disabled(2) it won't be used. You may also delete this entry by changing it to delete(3). Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH