>> MIB - Management Information Base
>> Table: sensorTable - (.1.3.6.1.4.1.272.4.17.7.1.1.1)
Description: This table contains all sensors of the system.
sensorTable
OID | Name | Type | Access
.1 | Slot | Unsigned32 | R
.2 | Number | Unsigned32 | R
.3 | Descr | DisplayString | R
.4 | Type | ENUM | R
.5 | Value | INTEGER | R
.7 | MeasurementUnit | DisplayString | R
Slot
Slot where sensor is placed.
Number
A unique number for a sensor in the slot.
Descr
Decscription of sensor. Length: 0 to 255
Type
Type of sensor. Enumerations: temperature (1) fanspeed (2) voltage (3)
Value
Current value of sensor.
MeasurementUnit
Unit of Value. Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH