>> MIB - Management Information Base
>> Table: memoryTable - (.1.3.6.1.4.1.272.4.17.4.2.1)
Description: The memoryTable contains information about the different memory in the system.
memoryTable
OID | Name | Type | Access
.1 | Type | ENUM | R
.2 | Descr | DisplayString | R
.3 | BlockSize | Unsigned32 | R
.4 | Total | Unsigned32 | R
.5 | Inuse | Unsigned32 | R
.6 | DramUse | Unsigned32 | R
.7 | NAllocs | Unsigned32 | R
.8 | NFrees | Unsigned32 | R
.9 | NFails | Unsigned32 | R
Type
Type of memory: flash (1) : Non volatile memory dram (2) : Dynamic memory dpool (3) : Dynamic pool Enumerations: flash (1) dram (2) dpool (3)
Descr
Description of memory. Length: 0 to 255
BlockSize
Allocation size for memories from dpools.
Total
Amount of available units of this memory type measured in units for dpools and bytes for flash/dram.
Inuse
Used units of this memory type measured in units for dpools and bytes for flash/dram.
DramUse
dpools might take memory from dram. This variable gives the amount in bytes taken from a dram memory.
NAllocs
Number of memory allocations.
NFrees
Number of memory free operations.
NFails
Number of failed memory operations.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH