>> MIB - Management Information Base
>> Table: certCacheStats - (.1.3.6.1.4.1.272.4.26.33.8.64)
certCacheStats
OID | Name | Type | Access
.1 | MemoryUsage | INTEGER | R
.2 | NumEntries | INTEGER | R
.3 | NumCertCacheHit | INTEGER | R
.4 | NumCertCacheMiss | INTEGER | R
.5 | NumCrlCacheHit | INTEGER | R
.6 | NumCrlCacheMiss | INTEGER | R
MemoryUsage
Allocated memory by the certificate cache.
NumEntries
Number of entries used in the certificate cache. Range: 0 to 65535
NumCertCacheHit
Number of successful certificate requests from cache. Range: 0 to 65535
NumCertCacheMiss
Number of failed certificate requests from cache. Range: 0 to 65535
NumCrlCacheHit
Number of successful crl requests from cache. Range: 0 to 65535
NumCrlCacheMiss
Number of failed crl requests from cache. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH