>> MIB - Management Information Base
>> Table: mpsTerminalStatusTable - (.1.3.6.1.4.1.272.4.53.14.3.1)
Description: This table contains the status information about IP terminal registered via Provisioning-Server.
mpsTerminalStatusTable
OID | Name | Type | Access
.1 | MacAddress | MacAddress | R
.2 | DeviceType | DisplayString | R
.3 | ContactURI | DisplayString | R
.4 | LastSeen | Date | R
.5 | SerialNr | DisplayString | R
.6 | SoftwareVersion | DisplayString | R
.7 | ConfigDate | Date | R
.8 | OEMType | ENUM | R
MacAddress
This variable contains the MAC address of the IP terminal. Length: 6 to 6
DeviceType
This variable contains device type of the terminal. Length: 0 to 255
ContactURI
This variable contains contact URI of the terminal: e.g. 'http://192.168.0.105:8085/contact_dls.html/ContactDLS' Length: 0 to 255
LastSeen
The date of last register at the provisioning server. Range: 0 to -1
SerialNr
This variable contains serial number of the terminal. Length: 0 to 255
SoftwareVersion
Software version of the IP terminal. Length: 0 to 20
ConfigDate
The date of last configuration change via the provisioning server. Range: 0 to -1
OEMType
OEM device type of the terminal e.g. Siemens OpenStage, Gigaset... Enumerations: none (1) openstage (2) gigaset (3)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH