>> MIB - Management Information Base
>> Table: lispCchEtrTable - (.1.3.6.1.4.1.272.4.23.9.7.1)
Description: List of cached ETRs for remote LISP-sites (see section 4.1 of RFC-6833 and section 4.1.4 of RFC-6830). In current implementation, support of multiple ETRs is rather restricted (no load-balancing, no reachability-checks).
lispCchEtrTable
OID | Name | Type | Access
.1 | InstId | INTEGER | R
.2 | SiteAddr | IpAddress | R
.3 | SiteLen | INTEGER | R
.4 | Addr | IpAddress | R
.5 | Prio | INTEGER | R
.6 | Weight | INTEGER | R
.7 | FlagL | ENUM | R
.8 | FlagR | ENUM | R
InstId
Refers to lispInstId-field of related lispCchSite-entry. Range: -1 to 16777215
SiteAddr
Refers to lispCchSiteAddr-field of related lispCchSite-entry.
SiteLen
Refers to lispCchSiteLen-field of related lispCchSite-entry. Range: 0 to 32
Addr
RLOC of this cached remote ETR.
Prio
Prio of this cached remote ETR. See 6.1.4 of RFC-6830 for details. Range: 0 to 255
Weight
Weight of this cached remote ETR. See 6.1.4 of RFC-6830 for details. Current implementation mostly yet ignores this value. Range: 0 to 255
FlagL
Flag L of this cached remote ETR. See 6.1.4 of RFC-6830 for details. Current implementation mostly yet ignores this value. Enumerations: not-local (0) local (1)
FlagR
Flag R of this cached remote ETR. See 6.1.4 of RFC-6830 for details. Current implementation mostly yet ignores this value. Enumerations: has-no-route (0) has-route (1)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH