>> MIB - Management Information Base
>> Table: voipStatRtcpHistoryTable - (.1.3.6.1.4.1.272.4.33.22.4.1)
Description: Describes completed call specific statistics calculated from voipStatRtcpEntryTable
voipStatRtcpHistoryTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Reference | INTEGER | R
.3 | Date | Date | R
.4 | Duration | TimeTicks | R
.5 | AvgRoundTripDelay | INTEGER | R
.6 | LocalIdent | DisplayString | R
.7 | LocalAvgInterarrivalJitter | INTEGER | R
.8 | LocalPackets | INTEGER | R
.9 | LocalBytes | INTEGER | R
.10 | LocalPacketLossRate | INTEGER | R
.11 | RemoteIdent | DisplayString | R
.12 | RemoteAvgInterarrivalJitter | INTEGER | R
.13 | RemotePackets | INTEGER | R
.14 | RemoteBytes | INTEGER | R
.15 | RemotePacketLossRate | INTEGER | R
Index
Unique Index to reference this entry
Reference
Reference to the Account the local statistic belongs.
Date
The Starttime and date of the call. Range: 0 to -1
Duration
The Duration of the call.
AvgRoundTripDelay
Average round trip delay in microseconds taken from related voipStatRtcpEntry
LocalIdent
Local Source Description taken from voipStatRtcpEntry. Length: 0 to 255
LocalAvgInterarrivalJitter
Average receive interarrival jitter in microseconds taken from related voipStatRtcpEntry.
LocalPackets
Count of local generated RTP data Packets.
LocalBytes
Count of local generated RTP data bytes.
LocalPacketLossRate
Receive packet loss rate in percent taken from related voipStatRtcpEntry. Range: 0 to 100
RemoteIdent
Far-end Source Description taken from voipStatRtcpEntry. Length: 0 to 255
RemoteAvgInterarrivalJitter
Average far-end interarrival jitter in microseconds taken from related voipStatRtcpEntry.
RemotePackets
Count of far-end generated RTP data Packets taken from related voipStatRtcpEntry.
RemoteBytes
Current count of far-end generated RTP data bytes taken from related voipStatRtcpEntry.
RemotePacketLossRate
Far end receive packet lost rate in percent taken from related voipStatRtcpEntry. Range: 0 to 100

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH