>> MIB - Management Information Base
>> Table: biboAdmLicInfoTable - (.1.3.6.1.4.1.272.4.1.32.1)
Description: This table contains an entry for each feature, that can be activated by a license. The licenses have to be entered in the biboAdmLicenseTable. This tabl indicates the current state of the different licenses.
biboAdmLicInfoTable
OID | Name | Type | Access
.1 | Type | ENUM | R
.2 | Status | ENUM | R
.3 | Id | DisplayString | R
.4 | Slot | INTEGER | R
.5 | MaxLic | Counter32 | R
.6 | InUse | Counter32 | R
.7 | HwSerial | DisplayString | R
.8 | Unit | INTEGER | R
.9 | Limit | Counter32 | R
.10 | Free | Counter32 | R
Type
The licenseable feature. Enumerations: ip (1) capi (2) bridge (3) x25 (4) ipx (5) stac (6) frame-relay (7) tapi (8) ospf (9) extended-lan (10) tunneling (11) taf (12) extended-wan (13) leased-line (14) lcr (15) app-power-phone (17) app-operator-desk (18) app-voice-mail-server (19) app-accounting-tool (20) app-intelligent-voice (21) app-6 (22) e25 (29) ipsec (33) ipseccb-ipxfer (34) bgp (35) uefs (36) siplan (37) siptrunk (38) pim (39) call-by-call (40) fax (41) sipout (42) brrp (43) wlan-controller (44) terminal-option (45) ethernet (128) bri (129) g703 (130) pri (131) modem (132) g7032pri (133) slots (134) e3 (135) serial (136) shdsl (137)
Status
The current state of the license. Enumerations: builtin (1) valid-license (2) invalid-license (3) no-license (4) erase-internal (5)
Id
The complete serial id string of the special license. Range: 0 to 255
Slot
In case of a hardware license corresponding to a dedicated module serial number, it is the slot number of the module. Range: 0 to 255
MaxLic
The max number of allowed chunks.
InUse
The current number of chunks in use.
HwSerial
The complete serial id string of the special license. Range: 0 to 255
Unit
In case of a hardware license corresponding to a dedicated module serial number, it is the unit number of the module. Range: 0 to 255
Limit
The maximum number of licenseable chunks.
Free
The number of free default licences.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH