>> MIB - Management Information Base
>> Table: mpsTrunkGroupTable - (.1.3.6.1.4.1.272.4.53.3.3.1)
Description: This table contains global information of the external trunk groups.
mpsTrunkGroupTable
OID | Name | Type | Access
.1 | Index | TrunkGroupIndex | RW
.2 | Layer2AlwaysOn | ENUM | RW
.3 | DefaultTargetType | ENUM | RW
.4 | DefaultTargetGroupIndex | GroupIndexOrZero | RW
.5 | DefaultTargetExtensionIndex | ExtensionIndexOrZero | RW
.6 | AdminStatus | ENUM | D
Index
A unique value for each trunk group. Range: 1 to 65535
Layer2AlwaysOn
This value determine if the Layer2 for this external isdn port is always on (1) or off (2). Enumerations: true (1) false (2)
DefaultTargetType
This value contains the default target type at wrong dialing, default is group. Enumerations: group (1) extension (2)
DefaultTargetGroupIndex
This value contains the default target group index if the mpsTrunkGroupDefaultTargetType = group (1). Range: 0 to 99
DefaultTargetExtensionIndex
This value contains the default target extension index if the mpsTrunkGroupDefaultTargetType = extension(2). Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH