>> MIB - Management Information Base
>> Table: mpsExtensionTable - (.1.3.6.1.4.1.272.4.53.6.1.1)
Description: This table contains all internal extensions.
mpsExtensionTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | IfIndex | InterfaceIndexOrZero | RW
.3 | DeviceVirtualIndex | INTEGER | RW
.4 | Number | DisplayString | RW
.5 | DisplayName | DisplayString | RW
.6 | AuthName | DisplayString | RW
.7 | AdminStatus | ENUM | D
Index
A unique value for each internal extension. Range: 1 to 65535
IfIndex
InterfaceIndex where the extension is placed. Range: 0 to 2147483647
DeviceVirtualIndex
This value contains the virtual device index of the mpsDeviceVirtual table, if the mpsExtensionIfIndex is zero.
Number
This value contains the internal number for the extension. Range: 0 to 4
DisplayName
Internal name of the extension. This name will be displayed at the internal calling party. Range: 0 to 20
AuthName
Login name for VoIP-registration at the pbx. Range: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH