>> MIB - Management Information Base
>> Table: mpsGroupTable - (.1.3.6.1.4.1.272.4.53.5.1.1)
Description: This table contains the information of the global team parameter for each extension group.
mpsGroupTable
OID | Name | Type | Access
.1 | Index | GroupIndex | RW
.2 | DisplayName | DisplayString | RW
.3 | Number | DisplayString | RW
.4 | NoReplyTimeout | INTEGER | RW
.5 | MulticastTrigger | INTEGER | RW
.6 | CallForwardingEnable | ENUM | RW
.7 | CallCalendar | INTEGER | RW
.8 | AdminStatus | ENUM | D
Index
A unique value for each group. Range: 1 to 99
DisplayName
Internal name of the group. Range: 0 to 20
Number
This value contains the extension number of the group. Allowing all group members to be reached at all times for external and internal calls Range: 0 to 4
NoReplyTimeout
The linear and rotating team calls allow you to configure a time interval in seconds, after which the next member of the team will be called.
MulticastTrigger
The linear and rotating team calls allow you to configure a time interval in seconds, after which all members of the team will be called at the same time.
CallForwardingEnable
This value determine if call forwarding of the extension group member will be done(1) or not(2). Enumerations: true (1) false (2)
CallCalendar
Select a calendar to switch the call mode automatically. After you have selected a calendar you can set the active call mode. 0 (not active), 1 (day mode), 2 (night mode).
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH