>> MIB - Management Information Base
>> Table: mpsArsRoutingDetailsTable - (.1.3.6.1.4.1.272.4.53.10.5.1)
Description: This table assigns a carrier and start time selection to an entry in the mpsArsRoutingTable.
mpsArsRoutingDetailsTable
OID | Name | Type | Access
.1 | Hour | INTEGER | RW
.2 | Minute | INTEGER | RW
.3 | RoutingIndex | RouteIndex | RW
.4 | CarrierIndex | CarrierIndex | RW
.5 | AdminStatus | ENUM | D
Hour
THis object specifies the hour for the beginning of this routing entry to be active. Range: 0 to 23
Minute
Range: 0 to 59
RoutingIndex
This object specifies a Number for the LCR Zone.
CarrierIndex
A unique index for each carrier.
AdminStatus
Specifies whether this entry defines a LCR RoutingDetails Entry or should be deleted Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH