>> MIB - Management Information Base
>> Table: userAlertTable - (.1.3.6.1.4.1.272.4.43.1.1)
Description: Contents the notification Entry
userAlertTable
OID | Name | Type | Access
.1 | Address | DisplayString | RW
.2 | Rule | DisplayString | RW
.3 | Timeout | INTEGER | RW
.4 | Count | INTEGER | RW
.5 | Compress | ENUM | D
.6 | Level | ENUM | RW
.7 | Mask | INTEGER | RW
Address
The receiver of a notification Range: 0 to 80
Rule
The Description of the Content Filter Rule Range: 0 to 255
Timeout
The Timeout the email is forced to send Range: 0 to 86400
Count
The count of Messages the email is forced to send Range: 0 to 1024
Compress
Compressed notification of Messages. This Message was repeated xxTimes Enumerations: enable (1) disable (2) delete (3)
Level
The Level of Message watching. Enumerations: emerg (1) user (2) crit (3) err (4) warning (5) notice (6) info (7) debug (8)
Mask
The Subtypes of Message watching.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH