>> MIB - Management Information Base
>> Table: mpsSysCharge - (.1.3.6.1.4.1.272.4.53.1.3)
mpsSysCharge
OID | Name | Type | Access
.1 | Protocol | ENUM | RW
.2 | Frequency | ENUM | RW
.3 | IncomingCall | ENUM | RW
.4 | Multiplier | INTEGER | RW
.5 | Exponent | INTEGER | RW
.6 | CurrencyName | DisplayString | RW
.7 | ExtensionIndex | ExtensionIndexOrZero | RW
.8 | HiddenDigitsCountA | INTEGER | RW
.9 | HiddenDigitsCountB | INTEGER | RW
Protocol
This value determine the charging protocol on the internal isdn ports. You have three options here: Keypad protocol - Charge data is transferred such that it can be displayed directly by the terminal device. Functional protocol - Charge data is transferred with binary encoding and must be decoded by the terminal device. Both - Both of these protocols are recognized (default settings for the PABX system. Enumerations: keypad-and-functional (1) no-keypad (2) no-functional (3)
Frequency
This value determine the frequency of the charge pulse for analog extensions Enumerations: no (1) f12khz (2) f16khz (3)
IncomingCall
You can define whether acquisition is to be made for all connection (1), or only when a project number is input (2). Enumerations: true (1) false (2)
Multiplier
Charge rate multiplier
Exponent
Charge rate exponent.
CurrencyName
This name will be displayed at the extension. Range: 0 to 3
ExtensionIndex
You can define an extension index at which internal telephone the communication data overflow is to be signaled per uus1 message. Range: 0 to 65535
HiddenDigitsCountA
You can enter the number of hidden digit positions for incoming calls. The positions (numbers) are concealed from right to left (from the end of the number). -1 = hide all
HiddenDigitsCountB
You can enter the number of hidden digit positions for outcoming calls. The positions (numbers) are concealed from right to left (from the end of the number). -1 = hide all

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH