>> MIB - Management Information Base
>> Table: dot11WEPDefaultKeysTable - (.1.2.840.10036.1.3.1)
Description: An Entry (conceptual row) in the WEP Default Keys Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11WEPDefaultKeysTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Value | WEPKeytype | RW
Index
The auxiliary variable used to identify instances of the columnar objects in the WEP Default Keys Table. The value of this variable is equal to the WEPDefaultKeyID + 1 Range: 1 to 4
Value
A WEP default secret key value. Length: 5 to 5

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH