>> MIB - Management Information Base
>> Table: ipsecPublicKeyTable - (.1.3.6.1.4.1.272.4.26.2.1)
Description: This object contains a key pair for a certain public key algorithm and the ids used together with this key.
ipsecPublicKeyTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Description | DisplayString | RW
.3 | Algorithm | ENUM | D
.4 | KeyLength | INTEGER | RW
.5 | PublicExponent | INTEGER | RW
.6 | State | ENUM | R
Index
A unique index for this entry.
Description
An optional description for this key. Length: 0 to 255
Algorithm
This object specifies the algorithm for which the key is used. Possible values: rsa(2), -- The RSA encryption algorithm dsa(3), -- The digital signature algorithm delete(15) -- Mark this entry for deletion. Enumerations: rsa (2) dsa (3) delete (15)
KeyLength
The size of the public and private keys in bits.
PublicExponent
The RSA public exponent of the key. (undefined for DSA)
State
This object specifies the state of the Key. Possible values: generating(1), -- Key generation is in progress complete(2), -- Key generation is complete error(3) -- Key generation terminated with an error. Enumerations: generating (1) complete (2) error (3)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH