>> MIB - Management Information Base
>> Table: mobilePLMNTable - (.1.3.6.1.4.1.272.4.41.4.1.27.1)
Description: A single mobilePLMNTable entry.
mobilePLMNTable
OID | Name | Type | Access
.1 | Code | INTEGER | R
.2 | Name | DisplayString | R
Code
The PLMN (Public Land Mobile Network) code of the network operator. This code is merged from the MCC (Mobile Country Code) and MNC (Mobile Network Code) of the network operator.
Name
The name of the network operator. Length: 0 to 20

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH