>> MIB - Management Information Base
>> Table: cpuTable - (.1.3.6.1.4.1.272.4.17.4.1.1)
Description: The CpuTable contains information about the processor statistics in the system.
cpuTable
OID | Name | Type | Access
.1 | Number | INTEGER | R
.2 | Descr | DisplayString | R
.3 | TotalUser | INTEGER | R
.4 | TotalSystem | INTEGER | R
.5 | TotalStreams | INTEGER | R
.6 | TotalIdle | INTEGER | R
.7 | LoadUser | INTEGER | R
.8 | LoadSystem | INTEGER | R
.9 | LoadStreams | INTEGER | R
.10 | LoadIdle | INTEGER | R
.11 | LoadUser10s | INTEGER | R
.12 | LoadSystem10s | INTEGER | R
.13 | LoadStreams10s | INTEGER | R
.14 | LoadIdle10s | INTEGER | R
.15 | LoadUser60s | INTEGER | R
.16 | LoadSystem60s | INTEGER | R
.17 | LoadStreams60s | INTEGER | R
.18 | LoadIdle60s | INTEGER | R
Number
CPU Number.
Descr
Description of CPU. Length: 0 to 255
TotalUser
Total time in seconds spent in user mode since booting.
TotalSystem
Total time in seconds spent in sytem mode since booting.
TotalStreams
Total time in seconds spent with streams processing since booting.
TotalIdle
Total idle time in seconds since booting.
LoadUser
Percentage of time spent in user mode for the last second. Range: 0 to 100
LoadSystem
Percentage of time spent in system mode for the last second. Range: 0 to 100
LoadStreams
Percentage of time spent with streams processing for the last second. Range: 0 to 100
LoadIdle
Percentage of idle time for the last second. Range: 0 to 100
LoadUser10s
Percentage of time spent in user mode for the last 10 seconds. Range: 0 to 100
LoadSystem10s
Percentage of time spent in system mode for the last 10 seconds. Range: 0 to 100
LoadStreams10s
Percentage of time spent with streams processing for the last 10 seconds. Range: 0 to 100
LoadIdle10s
Percentage of idle time measured for the last 10 seconds. Range: 0 to 100
LoadUser60s
Percentage of time spent in user mode for the last 60 seconds. Range: 0 to 100
LoadSystem60s
Percentage of time spent in system mode for the last 60 seconds. Range: 0 to 100
LoadStreams60s
Percentage of time spent with streams processing for the last 60 seconds. Range: 0 to 100
LoadIdle60s
Percentage of idle time measured for the last 60 seconds. Range: 0 to 100

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH