>> MIB - Management Information Base
>> Table: mpsSysCalendarTable - (.1.3.6.1.4.1.272.4.53.1.4.1)
Description: This table contains information for each circuit switching time of the calendar.
mpsSysCalendarTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Day | ENUM | RW
.3 | Position | INTEGER | RW
.4 | Hour | INTEGER | RW
.5 | Minute | INTEGER | RW
.6 | Mode | GroupModeIndex | RW
.7 | AdminStatus | ENUM | D
Index
A unique value for each calendar.
Day
A unique value for each day of the calendar. Enumerations: monday (1) tuesday (2) wednesday (3) thursday (4) friday (5) saturday (6) sunday (7)
Position
A unique value for each calendar, day and position.
Hour
This variable contains the hour for the switching time.
Minute
This variable contains the minutes for the switching time.
Mode
This variable contains the mode, to which the calendar will be switched. Range: 1 to 10
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH