>> MIB - Management Information Base
>> Table: wlanACLDeniedTable - (.1.3.6.1.4.1.272.4.46.7.1)
Description: Contains all MAC Addresses of denied clients
wlanACLDeniedTable
OID | Name | Type | Access
.1 | Address | MacAddress | R
.2 | IfIndex | INTEGER | R
.3 | Count | INTEGER | R
.4 | Age | INTEGER | R
Address
The MAC Address of the denied Client Length: 6 to 6
IfIndex
The Interface the Deniued Address belongs to
Count
The count of detected denies to this MAC Address
Age
The Age of the last MAX-ACCESS

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH