>> MIB - Management Information Base
>> Table: sshcKnownHostTable - (.1.3.6.1.4.1.272.4.44.3.1)
Description: 'MIB-emulation' of 'known_hosts' files (see 'ssh' manual-page). Each entry represents one line-part of such a file (maximum line-length exceeds maximum MIB-string-length). Line-parts are concatenated internally in specified order. Multiple files can be defined in this table. SSH-client reads only such entries where 'sshcKnownHostFileName' matches with internal variables 'GlobalKnownHostsFile' or 'UserKnownHostsFile' and ignores any entries with non-matching file-name. For backwards-compatibility, if no entry has matching file-name, SSH-client skips any known-host-checks (allows any server). If at least one entry has matching file-name, SSH-client accepts only such SSH-servers that authenticate successfully against contents of emulated 'known_hosts' files. It does not accept any new or changed SSH-servers in this case. Current file-emulation allows only reading but no writing.
sshcKnownHostTable
OID | Name | Type | Access
.1 | FileName | DisplayString | RW
.2 | LineNumber | INTEGER | RW
.3 | PartNumber | INTEGER | RW
.4 | AdminStatus | ENUM | D
.5 | PartString | DisplayString | RW
FileName
Name of to-be-emulated known_host file where this entry belongs to. Length: 0 to 255
LineNumber
Line-number of this entry.
PartNumber
Part-number (within line) of this entry.
AdminStatus
Activate/deactivate/delete this entry. NOTE: when this status is set to 'delete' entries are not removed immediately but at next start of SSH-client. Enumerations: enabled (1) disabled (2) delete (3)
PartString
Contents of this line-entry. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH