>> MIB - Management Information Base
>> Table: pimStarStarRPITable - (.1.3.6.1.4.1.272.4.5.54.2.1.104.1)
Description: An entry (conceptual row) in the pimStarStarRPITable.
pimStarStarRPITable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | UpTime | TimeTicks | R
.3 | PrunePendingTimer | TimeTicks | R
.4 | JoinExpiryTimer | TimeTicks | R
.5 | JoinPruneState | ENUM | R
IfIndex
The ifIndex of the interface that this entry corresponds to. Range: 1 to 2147483647
UpTime
The time since this entry was created by the local router.
PrunePendingTimer
description not available
JoinExpiryTimer
description not available
JoinPruneState
The state resulting from (*,*,RP) Join/Prune messages received on this interface. This corresponds to the state of the downstream per-interface (*,*,RP) state machine in the PIM-SM specification. Enumerations: noInfo (1) join (2) prunePending (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH