>> MIB - Management Information Base
>> Table: ipSifAliasTable - (.1.3.6.1.4.1.272.4.5.30.1)
Description: Contains a Stateful Inspection Firewall (SIF) policy.
ipSifAliasTable
OID | Name | Type | Access
.1 | Order | INTEGER | RW
.2 | Source | INTEGER | RW
.3 | Destination | INTEGER | RW
.4 | Service | INTEGER | RW
.5 | Action | ENUM | D
.6 | Status | ENUM | RW
.7 | Priority | ENUM | RW
.8 | ClassId | INTEGER | RW
Order
The Order for the Stateful Inspection Entry rule
Source
The alias Source Index for the Entry
Destination
The alias Destination Index for the Entry
Service
The alias Protocol/service Index for Entry
Action
The Rule for the Filter Enumerations: access (1) deny (2) reject (3) delete (255)
Status
Defines the administrative status of this policy Enumerations: enabled (1) disabled (2)
Priority
Defines the QoS priority of this policy Enumerations: default (1) low-latency (2) high (3) medium (4) low (5)
ClassId
Internal ID for SIF policy to QoS policy mapping Range: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH