>> MIB - Management Information Base
>> Table: wlcACLProfileTable - (.1.3.6.1.4.1.272.4.61.1.21.1)
Description: This table contains different ACL profiles. The WLAN Access List is based on MAC Addresses.
wlcACLProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Address | MacAddress | RW
.3 | AdminStatus | ENUM | D
Index
The variable is the unique profile index.
Address
The MAC Address for the accepted client. Length: 6 to 6
AdminStatus
Enable, disable or delete the requested ACL profile entry. Enumerations: disabled (1) enabled (2) delete (32)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH