>> MIB - Management Information Base
>> Table: mpsFaxSwitchTable - (.1.3.6.1.4.1.272.4.53.11.1.1)
Description: This table contains the information about fax switches.
mpsFaxSwitchTable
OID | Name | Type | Access
.1 | Index | FaxSwitchIndex | RW
.2 | CallCalendar | INTEGER | RW
.3 | AdminStatus | ENUM | D
Index
A unique value for each fax switch. Use the same value in mpsFaxSwitchModeIndex and mpsFaxSwitchUserIndex as reference to this entry. Range: 1 to 65535
CallCalendar
Select a calendar to switch the fax mode automatically. The active mode will be set in mpsFaxSwitchUserModeNumber in mpsFaxSwitchUserTable.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH